	*************************************************
	*                                               *
	*                Mē+LBA Readme.txt              *
	*                 for version 1.xx              *
	*                                               *
	*************************************************

Contents

Section 0.  Known Bugs and How to Avoid Them.

Section 1.  Errata

Section 2.  Notes on Installing and Uninstalling Mē+LBA.


	*************************************************

Section 0.  Known Bugs and How to Avoid Them.

We're working hard to find and eliminate all the bugs in this
software.  However, as of this release we still have a few tough
bugs for which we have not found complete solutions.  The
following list details these bugs and offers recovery and work-
around methods:


	*************************************************

Section 1.  Errata

			>>>>--------NOTICE--------<<<<

You must own both Mē-200 and LBA-PC in order to use Mē+LBA.
You must install Mē-200 before you can use Mē+LBA.

			>>>>--------NOTICE--------<<<<

	*************************************************
Section 2.  Notes on Installing and Uninstalling M2+LBA.

2.1	M2-200 v4.15 and later

The M2+LBA software is installed as part of the M2-200 System beginning with M2-200 v4.15.  No additional steps are necessary.  To run M2+LBA click on the Start button, Programs | Spiricon | M2-200 | M2+LBA Utility.

2.2	M2-200 v3.61 to v4.11

The M2+LBA software was created after M2-200 v4.11.  Customers with earlier versions will be sent a separate installation for the M2+LBA software in a ZIP file or on CD.   

Note:	M2-200 must be installed before using M2+LBA.

To install M2+LBA from a CD, using Windows Explorer go to the M2+LBA directory on the CD, double-click on the Setup.exe program, and follow the prompts.  The M2+LBA software will be installed in the M2-200 installation directory and a link to the program will be inserted in the Start Menu | Programs | Spiricon | M2-200.  To run M2+LBA click on the Start button, Programs | Spiricon | M2-200 | M2+LBA Utility.

To install M2+LBA from a ZIP file, unzip the file to a temporary directory - be sure the Use folder names option is checked in order to place the files in the directories specified in the ZIP file.  Using Windows Explorer, go to the M2+LBA directory in the temporary directory, double-click on the Setup.exe program, and follow the prompts.  The M2+LBA software will be installed in the M2-200 installation directory and a link to the program will be inserted in the Start Menu | Programs | Spiricon | M2-200.  To run M2+LBA click on the Start button, Programs | Spiricon | M2-200 | M2+LBA Utility.
